Static Call Graph - [..\OBJ\LCD.axf]

# Static Call Graph for image ..\OBJ\LCD.axf

#<CALLGRAPH># ARM Linker, 5060183: Last Updated: Wed Dec 06 15:55:42 2023

### Maximum Stack Usage = 920 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ ctp_test ⇒ lcd_draw_bline ⇒ gui_fill_circle ⇒ gui_draw_hline ⇒ LCD_Fill ⇒ LCD_SetCursor ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte

### Mutually Recursive functions

- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - ADC3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - BusFault_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - CST3XX_Scan from cst3xx.o(.text) referenced from touch.o(.text)
  - DMA1_Channel1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel5_IRQHandler from updater.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel4_5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DebugMon_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FLASH_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FSMC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - GT911_Scan from gt911.o(.text) referenced from touch.o(.text)
  - HardFault_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - MemManage_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - NMI_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - Null_Scan from gt911.o(.text) referenced from touch.o(.text)
  - PVD_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - PendSV_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RCC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTCAlarm_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - Reset_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SDIO_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SVC_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SysTick_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SystemInit from system_stm32f10x.o(.text) referenced from startup_stm32f10x_hd.o(.text)
  - TAMPER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM3_IRQHandler from updater.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM6_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM7_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_BRK_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_TRG_COM_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_UP_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TP_Adjust from touch.o(.text) referenced from touch.o(.data)
  - TP_Init from touch.o(.text) referenced from touch.o(.data)
  - TP_Scan from touch.o(.text) referenced from touch.o(.data)
  - UART4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UART5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART1_IRQHandler from usart.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UsageFault_Handler from stm32f10x_it.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - WWDG_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f10x_hd.o(.text)
  - fputc from usart.o(.text) referenced from printfa.o(i.__0printf)
  - main from main.o(.text) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  main (Thumb, 928 bytes, Stack size 656 bytes, main.o(.text))
  [Stack]

  - Max Depth = 920
  - Call Chain = main ⇒ ctp_test ⇒ lcd_draw_bline ⇒ gui_fill_circle ⇒ gui_draw_hline ⇒ LCD_Fill ⇒ LCD_SetCursor ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> uart_init
  - >> sendicon
  - >> rtp_test
  - >> py_get_keynum
  - >> delay_ms
  - >> delay_init
  - >> ctp_test
  - >> W25QXX_Init
  - >> TIM3_Int_Init
  - >> TIM2_PWM_Init
  - >> Show_Str
  - >> ShowUI
  - >> SendPWMval
  - >> NVIC_Configuration
  - >> Load_Drow_Dialog
  - >> LCD_ShowString
  - >> LCD_ShowNum
  - >> LCD_Init
  - >> LCD_Clear
  - >> free
  - >> __2printf
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SystemInit (Thumb, 64 bytes, Stack size 8 bytes, system_stm32f10x.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = SystemInit ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClockTo72
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(.text)

  SystemCoreClockUpdate (Thumb, 86 bytes, Stack size 8 bytes, system_stm32f10x.o(.text), UNUSED)

  LCD_WR_REG (Thumb, 30 bytes, Stack size 8 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = LCD_WR_REG ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> SPI2_ReadWriteByte
  [Called By]
  - >> LCD_Set_Window
  - >> LCD_Scan_Dir
  - >> LCD_SetCursor
  - >> LCD_WriteRAM_Prepare
  - >> LCD_WriteReg
  - >> LCD_INIT_CODE

  LCD_WR_DATA (Thumb, 32 bytes, Stack size 16 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> SPI2_ReadWriteByte
  [Called By]
  - >> LCD_Set_Window
  - >> LCD_Scan_Dir
  - >> LCD_SetCursor
  - >> LCD_WriteReg
  - >> LCD_INIT_CODE

  LCD_INIT_CODE (Thumb, 430 bytes, Stack size 8 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = LCD_INIT_CODE ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> LCD_WR_DATA
  - >> LCD_WR_REG
  - >> delay_ms
  [Called By]
  - >> LCD_Init

  LCD_WriteRAM (Thumb, 40 bytes, Stack size 16 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = LCD_WriteRAM ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> SPI2_ReadWriteByte
  [Called By]
  - >> LCD_Color_Fill
  - >> LCD_Fill
  - >> LCD_DrawPoint
  - >> image_show

  LCD_WriteReg (Thumb, 16 bytes, Stack size 8 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = LCD_WriteReg ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> LCD_WR_DATA
  - >> LCD_WR_REG
  [Called By]
  - >> LCD_Scan_Dir

  LCD_WriteRAM_Prepare (Thumb, 6 bytes, Stack size 0 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = LCD_WriteRAM_Prepare ⇒ LCD_WR_REG ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> LCD_WR_REG
  [Called By]
  - >> LCD_Color_Fill
  - >> LCD_Fill
  - >> LCD_DrawPoint
  - >> sendicon
  - >> LCD_Clear
  - >> image_show

  opt_delay (Thumb, 8 bytes, Stack size 0 bytes, lcd.o(.text), UNUSED)
  [Calls]

  - >> opt_delay
  [Called By]
  - >> opt_delay

  LCD_SetCursor (Thumb, 76 bytes, Stack size 24 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = LCD_SetCursor ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> LCD_WR_DATA
  - >> LCD_WR_REG
  [Called By]
  - >> LCD_Color_Fill
  - >> LCD_Fill
  - >> LCD_DrawPoint

  LCD_Scan_Dir (Thumb, 186 bytes, Stack size 8 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = LCD_Scan_Dir ⇒ LCD_WriteReg ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> LCD_WriteReg
  - >> LCD_WR_DATA
  - >> LCD_WR_REG
  [Called By]
  - >> LCD_Display_Dir

  LCD_DrawPoint (Thumb, 20 bytes, Stack size 8 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> LCD_SetCursor
  - >> LCD_WriteRAM_Prepare
  - >> LCD_WriteRAM
  [Called By]
  - >> text_show_font
  - >> TP_Draw_Big_Point
  - >> TP_Drow_Touch_Point
  - >> LCD_ShowChar
  - >> Draw_Circle
  - >> LCD_DrawLine

  LCD_Display_Dir (Thumb, 62 bytes, Stack size 16 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = LCD_Display_Dir ⇒ LCD_Scan_Dir ⇒ LCD_WriteReg ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> LCD_Scan_Dir
  [Called By]
  - >> sendicon
  - >> LCD_Init

  SendPWMval (Thumb, 22 bytes, Stack size 0 bytes, lcd.o(.text))
  [Called By]

  - >> NVIC_PriorityGroupConfigSet
  - >> main
  - >> Update

  TIM2_PWM_Init (Thumb, 128 bytes, Stack size 0 bytes, lcd.o(.text))
  [Called By]

  - >> NVIC_PriorityGroupConfigSet
  - >> main

  LCD_Set_Window (Thumb, 90 bytes, Stack size 24 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = LCD_Set_Window ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> LCD_WR_DATA
  - >> LCD_WR_REG
  [Called By]
  - >> sendicon
  - >> LCD_Clear
  - >> image_show

  LCD_Clear (Thumb, 80 bytes, Stack size 32 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = LCD_Clear ⇒ LCD_Set_Window ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> SPI2_ReadWriteByte
  - >> LCD_Set_Window
  - >> LCD_WriteRAM_Prepare
  [Called By]
  - >> NVIC_PriorityGroupConfigSet
  - >> TP_Init
  - >> TP_Adjust
  - >> rtp_test
  - >> ctp_test
  - >> Load_Drow_Dialog
  - >> LCD_Init
  - >> main

  LCD_Init (Thumb, 216 bytes, Stack size 24 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = LCD_Init ⇒ image_display ⇒ image_show ⇒ LCD_Set_Window ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> image_display
  - >> SPI2_Init
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_PinRemapConfig
  - >> GPIO_Init
  - >> LCD_Display_Dir
  - >> LCD_INIT_CODE
  - >> delay_ms
  - >> LCD_Clear
  [Called By]
  - >> NVIC_PriorityGroupConfigSet
  - >> main

  LCD_Fill (Thumb, 64 bytes, Stack size 32 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = LCD_Fill ⇒ LCD_SetCursor ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> LCD_SetCursor
  - >> LCD_WriteRAM_Prepare
  - >> LCD_WriteRAM
  [Called By]
  - >> gui_draw_hline

  LCD_Color_Fill (Thumb, 82 bytes, Stack size 32 bytes, lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_SetCursor
  - >> LCD_WriteRAM_Prepare
  - >> LCD_WriteRAM

  LCD_DrawLine (Thumb, 152 bytes, Stack size 48 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = LCD_DrawLine ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> LCD_DrawPoint
  [Called By]
  - >> TP_Drow_Touch_Point
  - >> LCD_DrawRectangle

  LCD_DrawRectangle (Thumb, 68 bytes, Stack size 32 bytes, lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_DrawLine

  Draw_Circle (Thumb, 196 bytes, Stack size 64 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = Draw_Circle ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> LCD_DrawPoint
  [Called By]
  - >> TP_Drow_Touch_Point

  LCD_ShowChar (Thumb, 222 bytes, Stack size 48 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> LCD_DrawPoint
  [Called By]
  - >> LCD_ShowxNum
  - >> Show_Str
  - >> LCD_ShowString
  - >> LCD_ShowNum

  LCD_Pow (Thumb, 16 bytes, Stack size 0 bytes, lcd.o(.text))
  [Called By]

  - >> LCD_ShowxNum
  - >> LCD_ShowNum

  LCD_ShowNum (Thumb, 112 bytes, Stack size 64 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 176
  - Call Chain = LCD_ShowNum ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> LCD_Pow
  - >> LCD_ShowChar
  [Called By]
  - >> TP_Adj_Info_Show
  - >> main

  LCD_ShowxNum (Thumb, 134 bytes, Stack size 64 bytes, lcd.o(.text), UNUSED)
  [Calls]

  - >> LCD_Pow
  - >> LCD_ShowChar

  LCD_ShowString (Thumb, 84 bytes, Stack size 48 bytes, lcd.o(.text))
  [Stack]

  - Max Depth = 160
  - Call Chain = LCD_ShowString ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> LCD_ShowChar
  [Called By]
  - >> TP_Adjust
  - >> TP_Adj_Info_Show
  - >> Load_Drow_Dialog
  - >> main
  - >> Update

  TP_Write_Byte (Thumb, 60 bytes, Stack size 24 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = TP_Write_Byte
  [Calls]
  - >> delay_us
  [Called By]
  - >> TP_Read_AD

  TP_Read_AD (Thumb, 124 bytes, Stack size 32 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = TP_Read_AD ⇒ TP_Write_Byte
  [Calls]
  - >> delay_us
  - >> TP_Write_Byte
  [Called By]
  - >> TP_Read_XOY

  TP_Read_XOY (Thumb, 96 bytes, Stack size 32 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = TP_Read_XOY ⇒ TP_Read_AD ⇒ TP_Write_Byte
  [Calls]
  - >> TP_Read_AD
  [Called By]
  - >> TP_Read_XY

  TP_Read_XY (Thumb, 36 bytes, Stack size 24 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = TP_Read_XY ⇒ TP_Read_XOY ⇒ TP_Read_AD ⇒ TP_Write_Byte
  [Calls]
  - >> TP_Read_XOY
  [Called By]
  - >> TP_Init
  - >> TP_Read_XY2

  TP_Read_XY2 (Thumb, 124 bytes, Stack size 40 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 152
  - Call Chain = TP_Read_XY2 ⇒ TP_Read_XY ⇒ TP_Read_XOY ⇒ TP_Read_AD ⇒ TP_Write_Byte
  [Calls]
  - >> TP_Read_XY
  [Called By]
  - >> TP_Scan

  TP_Drow_Touch_Point (Thumb, 130 bytes, Stack size 32 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 160
  - Call Chain = TP_Drow_Touch_Point ⇒ Draw_Circle ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> Draw_Circle
  - >> LCD_DrawLine
  - >> LCD_DrawPoint
  [Called By]
  - >> TP_Adjust

  TP_Draw_Big_Point (Thumb, 58 bytes, Stack size 24 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = TP_Draw_Big_Point ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> LCD_DrawPoint
  [Called By]
  - >> rtp_test

  TP_Scan (Thumb, 194 bytes, Stack size 16 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 168
  - Call Chain = TP_Scan ⇒ TP_Read_XY2 ⇒ TP_Read_XY ⇒ TP_Read_XOY ⇒ TP_Read_AD ⇒ TP_Write_Byte
  [Calls]
  - >> __aeabi_ui2f
  - >> __aeabi_i2f
  - >> __aeabi_fmul
  - >> __aeabi_fadd
  - >> __aeabi_f2uiz
  - >> TP_Read_XY2
  - >> __2printf
  [Address Reference Count : 1]
  - touch.o(.data)

  TP_Save_Adjdata (Thumb, 226 bytes, Stack size 16 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 136
  - Call Chain = TP_Save_Adjdata ⇒ W25QXX_Write ⇒ W25QXX_Write_NoCheck ⇒ W25QXX_Write_Page ⇒ W25QXX_Wait_Busy ⇒ W25QXX_ReadSR ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> __aeabi_fmul
  - >> __aeabi_f2iz
  - >> W25QXX_Write
  [Called By]
  - >> TP_Init
  - >> TP_Adjust

  TP_Get_Adjdata (Thumb, 236 bytes, Stack size 16 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = TP_Get_Adjdata ⇒ W25QXX_Read ⇒ DMA1_Spi1_RX
  [Calls]
  - >> __aeabi_i2f
  - >> __aeabi_fdiv
  - >> W25QXX_Read
  - >> __2printf
  [Called By]
  - >> TP_Init
  - >> TP_Adjust

  TP_Adj_Info_Show (Thumb, 360 bytes, Stack size 64 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 240
  - Call Chain = TP_Adj_Info_Show ⇒ LCD_ShowNum ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> LCD_ShowString
  - >> LCD_ShowNum
  [Called By]
  - >> TP_Adjust

  TP_Adjust (Thumb, 1446 bytes, Stack size 80 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 320
  - Call Chain = TP_Adjust ⇒ TP_Adj_Info_Show ⇒ LCD_ShowNum ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> __aeabi_ui2f
  - >> __aeabi_ui2d
  - >> __aeabi_i2f
  - >> __aeabi_fsub
  - >> __aeabi_fmul
  - >> __aeabi_fdiv
  - >> __aeabi_f2iz
  - >> __aeabi_f2d
  - >> __aeabi_dmul
  - >> __aeabi_d2uiz
  - >> __aeabi_cdrcmple
  - >> __aeabi_cdcmple
  - >> __ARM_scalbnf
  - >> TP_Adj_Info_Show
  - >> TP_Get_Adjdata
  - >> TP_Save_Adjdata
  - >> TP_Drow_Touch_Point
  - >> delay_ms
  - >> LCD_ShowString
  - >> LCD_Clear
  - >> __2printf
  - >> sqrt
  [Called By]
  - >> TP_Init
  [Address Reference Count : 1]
  - touch.o(.data)

  TP_Init (Thumb, 402 bytes, Stack size 32 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 352
  - Call Chain = TP_Init ⇒ TP_Adjust ⇒ TP_Adj_Info_Show ⇒ LCD_ShowNum ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> GT911_Init
  - >> GPIO_ResetBits
  - >> CST3XX_Init
  - >> TP_Adjust
  - >> TP_Get_Adjdata
  - >> TP_Save_Adjdata
  - >> TP_Read_XY
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_Init
  - >> W25QXX_Init
  - >> LCD_Clear
  [Address Reference Count : 1]
  - touch.o(.data)

  Is_In_Area (Thumb, 70 bytes, Stack size 24 bytes, touch.o(.text), UNUSED)
  [Calls]

  - >> delay_ms

  py_get_keynum (Thumb, 172 bytes, Stack size 32 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = py_get_keynum
  [Called By]
  - >> main

  Load_Drow_Dialog (Thumb, 70 bytes, Stack size 32 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 192
  - Call Chain = Load_Drow_Dialog ⇒ Show_Str ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> Show_Str
  - >> LCD_ShowString
  - >> LCD_Clear
  [Called By]
  - >> rtp_test
  - >> ctp_test
  - >> main

  ShowUI (Thumb, 80 bytes, Stack size 40 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 200
  - Call Chain = ShowUI ⇒ Show_Str ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> Show_Str
  [Called By]
  - >> rtp_test
  - >> ctp_test
  - >> main

  gui_draw_hline (Thumb, 22 bytes, Stack size 8 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = gui_draw_hline ⇒ LCD_Fill ⇒ LCD_SetCursor ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> LCD_Fill
  [Called By]
  - >> gui_fill_circle

  gui_fill_circle (Thumb, 182 bytes, Stack size 56 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 152
  - Call Chain = gui_fill_circle ⇒ gui_draw_hline ⇒ LCD_Fill ⇒ LCD_SetCursor ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> gui_draw_hline
  [Called By]
  - >> lcd_draw_bline

  my_abs (Thumb, 14 bytes, Stack size 0 bytes, touch.o(.text), UNUSED)

  lcd_draw_bline (Thumb, 172 bytes, Stack size 48 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 200
  - Call Chain = lcd_draw_bline ⇒ gui_fill_circle ⇒ gui_draw_hline ⇒ LCD_Fill ⇒ LCD_SetCursor ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> gui_fill_circle
  [Called By]
  - >> ctp_test

  ctp_test (Thumb, 282 bytes, Stack size 64 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 264
  - Call Chain = ctp_test ⇒ lcd_draw_bline ⇒ gui_fill_circle ⇒ gui_draw_hline ⇒ LCD_Fill ⇒ LCD_SetCursor ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> lcd_draw_bline
  - >> delay_ms
  - >> ShowUI
  - >> Load_Drow_Dialog
  - >> LCD_Clear
  - >> __2printf
  [Called By]
  - >> main

  rtp_test (Thumb, 98 bytes, Stack size 16 bytes, touch.o(.text))
  [Stack]

  - Max Depth = 216
  - Call Chain = rtp_test ⇒ ShowUI ⇒ Show_Str ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> TP_Draw_Big_Point
  - >> delay_ms
  - >> ShowUI
  - >> Load_Drow_Dialog
  - >> LCD_Clear
  [Called By]
  - >> main

  GT911_WR_Reg (Thumb, 82 bytes, Stack size 24 bytes, gt911.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = GT911_WR_Reg ⇒ CT_IIC_Wait_Ack ⇒ CT_IIC_Stop
  [Calls]
  - >> CT_IIC_Wait_Ack
  - >> CT_IIC_Stop
  - >> CT_IIC_Start
  - >> CT_IIC_Send_Byte
  [Called By]
  - >> GT911_Scan
  - >> GT911_Init

  GT911_RD_Reg (Thumb, 96 bytes, Stack size 24 bytes, gt911.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = GT911_RD_Reg ⇒ CT_IIC_Read_Byte ⇒ CT_IIC_NAck
  [Calls]
  - >> CT_IIC_Wait_Ack
  - >> CT_IIC_Stop
  - >> CT_IIC_Start
  - >> CT_IIC_Send_Byte
  - >> CT_IIC_Read_Byte
  [Called By]
  - >> GT911_Scan
  - >> GT911_Init

  GT911_Init (Thumb, 222 bytes, Stack size 32 bytes, gt911.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = GT911_Init ⇒ GT911_RD_Reg ⇒ CT_IIC_Read_Byte ⇒ CT_IIC_NAck
  [Calls]
  - >> CT_IIC_Init
  - >> GT911_RD_Reg
  - >> GT911_WR_Reg
  - >> GPIO_ResetBits
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_Init
  - >> delay_ms
  - >> __2printf
  - >> strcmp
  [Called By]
  - >> TP_Init

  GT911_Scan (Thumb, 328 bytes, Stack size 56 bytes, gt911.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = GT911_Scan ⇒ GT911_RD_Reg ⇒ CT_IIC_Read_Byte ⇒ CT_IIC_NAck
  [Calls]
  - >> GT911_RD_Reg
  - >> GT911_WR_Reg
  - >> __2printf
  [Address Reference Count : 1]
  - touch.o(.text)

  Null_Scan (Thumb, 4 bytes, Stack size 0 bytes, gt911.o(.text))
  [Address Reference Count : 1]

  - touch.o(.text)

  CT_Delay (Thumb, 6 bytes, Stack size 0 bytes, ctiic.o(.text), UNUSED)
  [Calls]

  - >> delay_us

  CT_IIC_Init (Thumb, 86 bytes, Stack size 16 bytes, ctiic.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = CT_IIC_Init ⇒ GPIO_Init
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_Init
  [Called By]
  - >> GT911_Init
  - >> CST3XX_Init

  CT_IIC_Start (Thumb, 56 bytes, Stack size 16 bytes, ctiic.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = CT_IIC_Start
  [Calls]
  - >> delay_us
  [Called By]
  - >> CST3XX_RD_Reg
  - >> CST3XX_WR_Reg
  - >> GT911_RD_Reg
  - >> GT911_WR_Reg

  CT_IIC_Stop (Thumb, 56 bytes, Stack size 16 bytes, ctiic.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = CT_IIC_Stop
  [Calls]
  - >> delay_us
  [Called By]
  - >> CST3XX_RD_Reg
  - >> CST3XX_WR_Reg
  - >> CT_IIC_Wait_Ack
  - >> GT911_RD_Reg
  - >> GT911_WR_Reg

  CT_IIC_Wait_Ack (Thumb, 78 bytes, Stack size 16 bytes, ctiic.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = CT_IIC_Wait_Ack ⇒ CT_IIC_Stop
  [Calls]
  - >> CT_IIC_Stop
  - >> delay_us
  [Called By]
  - >> CST3XX_RD_Reg
  - >> CST3XX_WR_Reg
  - >> GT911_RD_Reg
  - >> GT911_WR_Reg

  CT_IIC_Ack (Thumb, 56 bytes, Stack size 16 bytes, ctiic.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = CT_IIC_Ack
  [Calls]
  - >> delay_us
  [Called By]
  - >> CT_IIC_Read_Byte

  CT_IIC_NAck (Thumb, 56 bytes, Stack size 16 bytes, ctiic.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = CT_IIC_NAck
  [Calls]
  - >> delay_us
  [Called By]
  - >> CT_IIC_Read_Byte

  CT_IIC_Send_Byte (Thumb, 80 bytes, Stack size 24 bytes, ctiic.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = CT_IIC_Send_Byte
  [Calls]
  - >> delay_us
  [Called By]
  - >> CST3XX_RD_Reg
  - >> CST3XX_WR_Reg
  - >> GT911_RD_Reg
  - >> GT911_WR_Reg

  CT_IIC_Read_Byte (Thumb, 94 bytes, Stack size 32 bytes, ctiic.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = CT_IIC_Read_Byte ⇒ CT_IIC_NAck
  [Calls]
  - >> CT_IIC_NAck
  - >> CT_IIC_Ack
  - >> delay_us
  [Called By]
  - >> CST3XX_RD_Reg
  - >> GT911_RD_Reg

  W25QXX_ReadID (Thumb, 62 bytes, Stack size 16 bytes, w25qxx.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = W25QXX_ReadID ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> SPI1_ReadWriteByte
  [Called By]
  - >> W25QXX_Init

  W25QXX_Init (Thumb, 78 bytes, Stack size 16 bytes, w25qxx.o(.text))
  [Stack]

  - Max Depth = 132
  - Call Chain = W25QXX_Init ⇒ SPI1_Init ⇒ DMA1_Spi1_Init ⇒ DMA_Init
  [Calls]
  - >> SPI1_SetSpeed
  - >> SPI1_Init
  - >> W25QXX_ReadID
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_Init
  - >> __2printf
  [Called By]
  - >> NVIC_PriorityGroupConfigSet
  - >> TP_Init
  - >> main

  W25QXX_ReadSR (Thumb, 32 bytes, Stack size 8 bytes, w25qxx.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = W25QXX_ReadSR ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> SPI1_ReadWriteByte
  [Called By]
  - >> W25QXX_Wait_Busy

  W25QXX_Write_SR (Thumb, 34 bytes, Stack size 16 bytes, w25qxx.o(.text), UNUSED)
  [Calls]

  - >> SPI1_ReadWriteByte

  W25QXX_Write_Enable (Thumb, 26 bytes, Stack size 8 bytes, w25qxx.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = W25QXX_Write_Enable ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> SPI1_ReadWriteByte
  [Called By]
  - >> W25QXX_Erase_Chip
  - >> W25QXX_Erase_Sector
  - >> W25QXX_Write_Page

  W25QXX_Write_Disable (Thumb, 26 bytes, Stack size 8 bytes, w25qxx.o(.text), UNUSED)
  [Calls]

  - >> SPI1_ReadWriteByte

  W25QXX_Read (Thumb, 66 bytes, Stack size 24 bytes, w25qxx.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = W25QXX_Read ⇒ DMA1_Spi1_RX
  [Calls]
  - >> SPI1_ReadWriteByte
  - >> DMA1_Spi1_RX
  [Called By]
  - >> NVIC_PriorityGroupConfigSet
  - >> text_get_hz_mat
  - >> W25QXX_Write
  - >> TP_Get_Adjdata
  - >> sendicon
  - >> Update

  W25QXX_Wait_Busy (Thumb, 12 bytes, Stack size 8 bytes, w25qxx.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = W25QXX_Wait_Busy ⇒ W25QXX_ReadSR ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> W25QXX_ReadSR
  [Called By]
  - >> W25QXX_Erase_Chip
  - >> W25QXX_Erase_Sector
  - >> W25QXX_Write_Page

  W25QXX_Write_Page (Thumb, 80 bytes, Stack size 24 bytes, w25qxx.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = W25QXX_Write_Page ⇒ W25QXX_Wait_Busy ⇒ W25QXX_ReadSR ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> SPI1_ReadWriteByte
  - >> W25QXX_Wait_Busy
  - >> W25QXX_Write_Enable
  [Called By]
  - >> W25QXX_Write_NoCheck

  W25QXX_Write_NoCheck (Thumb, 60 bytes, Stack size 24 bytes, w25qxx.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = W25QXX_Write_NoCheck ⇒ W25QXX_Write_Page ⇒ W25QXX_Wait_Busy ⇒ W25QXX_ReadSR ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> W25QXX_Write_Page
  [Called By]
  - >> W25QXX_Write
  - >> Update

  W25QXX_Erase_Sector (Thumb, 62 bytes, Stack size 16 bytes, w25qxx.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = W25QXX_Erase_Sector ⇒ W25QXX_Wait_Busy ⇒ W25QXX_ReadSR ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> SPI1_ReadWriteByte
  - >> W25QXX_Wait_Busy
  - >> W25QXX_Write_Enable
  [Called By]
  - >> W25QXX_Write

  W25QXX_Write (Thumb, 150 bytes, Stack size 40 bytes, w25qxx.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = W25QXX_Write ⇒ W25QXX_Write_NoCheck ⇒ W25QXX_Write_Page ⇒ W25QXX_Wait_Busy ⇒ W25QXX_ReadSR ⇒ SPI1_ReadWriteByte
  [Calls]
  - >> W25QXX_Erase_Sector
  - >> W25QXX_Write_NoCheck
  - >> W25QXX_Read
  [Called By]
  - >> NVIC_PriorityGroupConfigSet
  - >> TP_Save_Adjdata
  - >> Update

  W25QXX_Erase_Chip (Thumb, 38 bytes, Stack size 8 bytes, w25qxx.o(.text), UNUSED)
  [Calls]

  - >> SPI1_ReadWriteByte
  - >> W25QXX_Wait_Busy
  - >> W25QXX_Write_Enable
  [Called By]
  - >> Update

  W25QXX_PowerDown (Thumb, 34 bytes, Stack size 8 bytes, w25qxx.o(.text), UNUSED)
  [Calls]

  - >> SPI1_ReadWriteByte
  - >> delay_us

  W25QXX_WAKEUP (Thumb, 34 bytes, Stack size 8 bytes, w25qxx.o(.text), UNUSED)
  [Calls]

  - >> SPI1_ReadWriteByte
  - >> delay_us

  sendicon (Thumb, 172 bytes, Stack size 56 bytes, w25qxx.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = sendicon ⇒ LCD_Display_Dir ⇒ LCD_Scan_Dir ⇒ LCD_WriteReg ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> W25QXX_Read
  - >> SPI2_ReadWriteByte
  - >> LCD_Set_Window
  - >> LCD_Display_Dir
  - >> LCD_WriteRAM_Prepare
  [Called By]
  - >> main

  DMA1_Spi1_Init (Thumb, 140 bytes, Stack size 72 bytes, spi1.o(.text))
  [Stack]

  - Max Depth = 84
  - Call Chain = DMA1_Spi1_Init ⇒ DMA_Init
  [Calls]
  - >> SPI_I2S_DMACmd
  - >> RCC_AHBPeriphClockCmd
  - >> DMA_Init
  - >> DMA_DeInit
  [Called By]
  - >> SPI1_Init

  SPI1_SetSpeed (Thumb, 26 bytes, Stack size 0 bytes, spi1.o(.text))
  [Calls]

  - >> SPI_Cmd
  [Called By]
  - >> SPI1_Init
  - >> W25QXX_Init

  SPI1_ReadWriteByte (Thumb, 78 bytes, Stack size 16 bytes, spi1.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = SPI1_ReadWriteByte
  [Calls]
  - >> SPI_I2S_SendData
  - >> SPI_I2S_ReceiveData
  - >> SPI_I2S_GetFlagStatus
  [Called By]
  - >> SPI1_Init
  - >> W25QXX_WAKEUP
  - >> W25QXX_PowerDown
  - >> W25QXX_Erase_Chip
  - >> W25QXX_Erase_Sector
  - >> W25QXX_Write_Page
  - >> W25QXX_Write_Disable
  - >> W25QXX_Write_Enable
  - >> W25QXX_Write_SR
  - >> W25QXX_ReadSR
  - >> W25QXX_ReadID
  - >> W25QXX_Read

  SPI1_Init (Thumb, 148 bytes, Stack size 32 bytes, spi1.o(.text))
  [Stack]

  - Max Depth = 116
  - Call Chain = SPI1_Init ⇒ DMA1_Spi1_Init ⇒ DMA_Init
  [Calls]
  - >> SPI_Init
  - >> SPI_Cmd
  - >> DMA1_Spi1_Init
  - >> SPI1_SetSpeed
  - >> SPI1_ReadWriteByte
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_Init
  [Called By]
  - >> W25QXX_Init

  DMA1_Spi1_RX (Thumb, 104 bytes, Stack size 24 bytes, spi1.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA1_Spi1_RX
  [Calls]
  - >> DMA_GetFlagStatus
  - >> DMA_Cmd
  - >> DMA_ClearFlag
  [Called By]
  - >> W25QXX_Read

  DMA1_Spi1_TX (Thumb, 52 bytes, Stack size 16 bytes, spi1.o(.text), UNUSED)
  [Calls]

  - >> DMA_GetFlagStatus
  - >> DMA_Cmd
  - >> DMA_ClearFlag

  SPI2_SetSpeed (Thumb, 24 bytes, Stack size 0 bytes, spi2.o(.text))
  [Calls]

  - >> SPI_Cmd
  [Called By]
  - >> SPI2_Init

  SPI2_ReadWriteByte (Thumb, 76 bytes, Stack size 16 bytes, spi2.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = SPI2_ReadWriteByte
  [Calls]
  - >> SPI_I2S_SendData
  - >> SPI_I2S_ReceiveData
  - >> SPI_I2S_GetFlagStatus
  [Called By]
  - >> SPI2_Init
  - >> LCD_WriteRAM
  - >> LCD_WR_DATA
  - >> LCD_WR_REG
  - >> sendicon
  - >> LCD_Clear

  SPI2_Init (Thumb, 144 bytes, Stack size 40 bytes, spi2.o(.text))
  [Stack]

  - Max Depth = 60
  - Call Chain = SPI2_Init ⇒ GPIO_Init
  [Calls]
  - >> RCC_APB1PeriphClockCmd
  - >> SPI2_SetSpeed
  - >> SPI_Init
  - >> SPI_Cmd
  - >> SPI2_ReadWriteByte
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_Init
  [Called By]
  - >> LCD_Init

  DMA1_Spi2_Init (Thumb, 140 bytes, Stack size 72 bytes, spi2.o(.text), UNUSED)
  [Calls]

  - >> SPI_I2S_DMACmd
  - >> RCC_AHBPeriphClockCmd
  - >> DMA_Init
  - >> DMA_DeInit

  DMA1_Spi2_RX (Thumb, 108 bytes, Stack size 24 bytes, spi2.o(.text), UNUSED)
  [Calls]

  - >> DMA_GetFlagStatus
  - >> DMA_Cmd
  - >> DMA_ClearFlag

  DMA1_Spi2_TX (Thumb, 54 bytes, Stack size 16 bytes, spi2.o(.text), UNUSED)
  [Calls]

  - >> DMA_GetFlagStatus
  - >> DMA_Cmd
  - >> DMA_ClearFlag

  text_show_font (Thumb, 162 bytes, Stack size 40 bytes, text.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = text_show_font ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> text_get_hz_mat
  - >> LCD_DrawPoint
  - >> malloc
  - >> free
  [Called By]
  - >> Show_Str

  Show_Str (Thumb, 172 bytes, Stack size 48 bytes, text.o(.text))
  [Stack]

  - Max Depth = 160
  - Call Chain = Show_Str ⇒ LCD_ShowChar ⇒ LCD_DrawPoint ⇒ LCD_SetCursor ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> text_show_font
  - >> LCD_ShowChar
  [Called By]
  - >> Show_Str_Mid
  - >> ShowUI
  - >> Load_Drow_Dialog
  - >> main

  Show_Str_Mid (Thumb, 88 bytes, Stack size 48 bytes, text.o(.text), UNUSED)
  [Calls]

  - >> Show_Str
  - >> strlen

  CST3XX_WR_Reg (Thumb, 84 bytes, Stack size 24 bytes, cst3xx.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = CST3XX_WR_Reg ⇒ CT_IIC_Wait_Ack ⇒ CT_IIC_Stop
  [Calls]
  - >> CT_IIC_Wait_Ack
  - >> CT_IIC_Stop
  - >> CT_IIC_Start
  - >> CT_IIC_Send_Byte
  [Called By]
  - >> CST3XX_Scan
  - >> CST3XX_Init

  CST3XX_RD_Reg (Thumb, 98 bytes, Stack size 24 bytes, cst3xx.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = CST3XX_RD_Reg ⇒ CT_IIC_Read_Byte ⇒ CT_IIC_NAck
  [Calls]
  - >> CT_IIC_Wait_Ack
  - >> CT_IIC_Stop
  - >> CT_IIC_Start
  - >> CT_IIC_Send_Byte
  - >> CT_IIC_Read_Byte
  [Called By]
  - >> CST3XX_Scan
  - >> CST3XX_Init

  CST3XX_Init (Thumb, 214 bytes, Stack size 24 bytes, cst3xx.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = CST3XX_Init ⇒ CST3XX_RD_Reg ⇒ CT_IIC_Read_Byte ⇒ CT_IIC_NAck
  [Calls]
  - >> CST3XX_RD_Reg
  - >> CST3XX_WR_Reg
  - >> CT_IIC_Init
  - >> GPIO_ResetBits
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_SetBits
  - >> GPIO_Init
  - >> delay_ms
  [Called By]
  - >> TP_Init

  CST3XX_Scan (Thumb, 328 bytes, Stack size 56 bytes, cst3xx.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = CST3XX_Scan ⇒ CST3XX_RD_Reg ⇒ CT_IIC_Read_Byte ⇒ CT_IIC_NAck
  [Calls]
  - >> CST3XX_RD_Reg
  - >> CST3XX_WR_Reg
  - >> __2printf
  [Address Reference Count : 1]
  - touch.o(.text)

  delay_init (Thumb, 46 bytes, Stack size 8 bytes, delay.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = delay_init
  [Calls]
  - >> SysTick_CLKSourceConfig
  [Called By]
  - >> main

  delay_us (Thumb, 46 bytes, Stack size 0 bytes, delay.o(.text))
  [Called By]

  - >> W25QXX_WAKEUP
  - >> W25QXX_PowerDown
  - >> CT_IIC_NAck
  - >> CT_IIC_Ack
  - >> CT_Delay
  - >> CT_IIC_Wait_Ack
  - >> CT_IIC_Stop
  - >> CT_IIC_Start
  - >> CT_IIC_Send_Byte
  - >> CT_IIC_Read_Byte
  - >> TP_Read_AD
  - >> TP_Write_Byte

  delay_ms (Thumb, 46 bytes, Stack size 0 bytes, delay.o(.text))
  [Called By]

  - >> NVIC_PriorityGroupConfigSet
  - >> GT911_Init
  - >> CST3XX_Init
  - >> Is_In_Area
  - >> TP_Adjust
  - >> LCD_INIT_CODE
  - >> rtp_test
  - >> ctp_test
  - >> LCD_Init
  - >> main

  NVIC_Configuration (Thumb, 18 bytes, Stack size 8 bytes, sys.o(.text))
  [Stack]

  - Max Depth = 172
  - Call Chain = NVIC_Configuration ⇒ NVIC_PriorityGroupConfigSet ⇒ W25QXX_Init ⇒ SPI1_Init ⇒ DMA1_Spi1_Init ⇒ DMA_Init
  [Calls]
  - >> NVIC_PriorityGroupConfigSet
  - >> NVIC_PriorityGroupConfig
  [Called By]
  - >> main

  _sys_exit (Thumb, 2 bytes, Stack size 0 bytes, usart.o(.text), UNUSED)

  fputc (Thumb, 18 bytes, Stack size 0 bytes, usart.o(.text))
  [Address Reference Count : 1]

  - printfa.o(i.__0printf)

  uart_init (Thumb, 156 bytes, Stack size 48 bytes, usart.o(.text))
  [Stack]

  - Max Depth = 92
  - Call Chain = uart_init ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> USART_Init
  - >> USART_ITConfig
  - >> USART_DeInit
  - >> USART_Cmd
  - >> NVIC_Init
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> NVIC_PriorityGroupConfigSet
  - >> main

  USART1_IRQHandler (Thumb, 102 bytes, Stack size 8 bytes, usart.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = USART1_IRQHandler ⇒ USART_GetITStatus
  [Calls]
  - >> USART_ReceiveData
  - >> USART_GetITStatus
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  ADC3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel4_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, misc.o(.text))
  [Called By]

  - >> NVIC_Configuration

  NVIC_Init (Thumb, 94 bytes, Stack size 12 bytes, misc.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = NVIC_Init
  [Called By]
  - >> uart_init
  - >> TIM3_Int_Init
  - >> USART1_RX_DMA_Init

  NVIC_SetVectorTable (Thumb, 14 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  NVIC_SystemLPConfig (Thumb, 20 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  SysTick_CLKSourceConfig (Thumb, 24 bytes, Stack size 0 bytes, misc.o(.text))
  [Called By]

  - >> delay_init

  GPIO_DeInit (Thumb, 152 bytes, Stack size 8 bytes, stm32f10x_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  GPIO_AFIODeInit (Thumb, 22 bytes, Stack size 8 bytes, stm32f10x_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  GPIO_Init (Thumb, 156 bytes, Stack size 20 bytes, stm32f10x_gpio.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_Init
  [Called By]
  - >> SPI1_Init
  - >> CT_IIC_Init
  - >> GT911_Init
  - >> CST3XX_Init
  - >> TP_Init
  - >> SPI2_Init
  - >> uart_init
  - >> W25QXX_Init
  - >> LCD_Init

  GPIO_StructInit (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadInputDataBit (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadInputData (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadOutputDataBit (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ReadOutputData (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text))
  [Called By]

  - >> SPI1_Init
  - >> CT_IIC_Init
  - >> GT911_Init
  - >> CST3XX_Init
  - >> TP_Init
  - >> SPI2_Init
  - >> W25QXX_Init
  - >> LCD_Init

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text))
  [Called By]

  - >> GT911_Init
  - >> CST3XX_Init
  - >> TP_Init

  GPIO_WriteBit (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_Write (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_PinLockConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EventOutputConfig (Thumb, 22 bytes, Stack size 8 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_EventOutputCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_PinRemapConfig (Thumb, 82 bytes, Stack size 20 bytes, stm32f10x_gpio.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_PinRemapConfig
  [Called By]
  - >> LCD_Init

  GPIO_EXTILineConfig (Thumb, 34 bytes, Stack size 8 bytes, stm32f10x_gpio.o(.text), UNUSED)

  GPIO_ETH_MediaInterfaceConfig (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_gpio.o(.text), UNUSED)

  RCC_DeInit (Thumb, 50 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HSEConfig (Thumb, 48 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetFlagStatus (Thumb, 42 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Called By]

  - >> RCC_WaitForHSEStartUp

  RCC_WaitForHSEStartUp (Thumb, 44 bytes, Stack size 12 bytes, stm32f10x_rcc.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetFlagStatus

  RCC_AdjustHSICalibrationValue (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PLLConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PLLCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_SYSCLKConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetSYSCLKSource (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_HCLKConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PCLK1Config (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_PCLK2Config (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ITConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_USBCLKConfig (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ADCCLKConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_LSEConfig (Thumb, 28 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_LSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_RTCCLKConfig (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_RTCCLKCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetClocksFreq (Thumb, 132 bytes, Stack size 12 bytes, stm32f10x_rcc.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = RCC_GetClocksFreq
  [Called By]
  - >> I2S_Init
  - >> USART_Init

  RCC_AHBPeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> DMA1_Spi2_Init
  - >> DMA1_Spi1_Init
  - >> USART1_RX_DMA_Init

  RCC_APB2PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> SPI1_Init
  - >> CT_IIC_Init
  - >> GT911_Init
  - >> CST3XX_Init
  - >> TP_Init
  - >> SPI2_Init
  - >> uart_init
  - >> W25QXX_Init
  - >> LCD_Init

  RCC_APB1PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> SPI2_Init
  - >> TIM3_Int_Init

  RCC_APB2PeriphResetCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> SPI_I2S_DeInit
  - >> GPIO_AFIODeInit
  - >> GPIO_DeInit
  - >> USART_DeInit
  - >> TIM_DeInit

  RCC_APB1PeriphResetCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text))
  [Called By]

  - >> SPI_I2S_DeInit
  - >> USART_DeInit
  - >> TIM_DeInit

  RCC_BackupResetCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClockSecuritySystemCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_MCOConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClearFlag (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_GetITStatus (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  RCC_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_rcc.o(.text), UNUSED)

  USART_DeInit (Thumb, 96 bytes, Stack size 8 bytes, stm32f10x_usart.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USART_DeInit
  [Calls]
  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB2PeriphResetCmd
  [Called By]
  - >> uart_init

  USART_Init (Thumb, 166 bytes, Stack size 32 bytes, stm32f10x_usart.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> uart_init

  USART_StructInit (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ClockInit (Thumb, 30 bytes, Stack size 8 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ClockStructInit (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text))
  [Called By]

  - >> uart_init

  USART_ITConfig (Thumb, 48 bytes, Stack size 8 bytes, stm32f10x_usart.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USART_ITConfig
  [Called By]
  - >> uart_init

  USART_DMACmd (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text))
  [Called By]

  - >> USART1_RX_DMA_Init

  USART_SetAddress (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_WakeUpConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ReceiverWakeUpCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_LINBreakDetectLengthConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_LINCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ReceiveData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text))
  [Called By]

  - >> USART1_IRQHandler

  USART_SendBreak (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SetGuardTime (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SetPrescaler (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SmartCardCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_SmartCardNACKCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_HalfDuplexCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_OverSampling8Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_OneBitMethodCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_IrDAConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_IrDACmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_GetFlagStatus (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  USART_GetITStatus (Thumb, 62 bytes, Stack size 16 bytes, stm32f10x_usart.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = USART_GetITStatus
  [Called By]
  - >> USART1_IRQHandler

  USART_ClearITPendingBit (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_usart.o(.text), UNUSED)

  SPI_I2S_DeInit (Thumb, 72 bytes, Stack size 8 bytes, stm32f10x_spi.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB2PeriphResetCmd

  SPI_Init (Thumb, 56 bytes, Stack size 12 bytes, stm32f10x_spi.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SPI_Init
  [Called By]
  - >> SPI1_Init
  - >> SPI2_Init

  I2S_Init (Thumb, 150 bytes, Stack size 40 bytes, stm32f10x_spi.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetClocksFreq

  SPI_StructInit (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  I2S_StructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text))
  [Called By]

  - >> SPI2_SetSpeed
  - >> SPI1_SetSpeed
  - >> SPI1_Init
  - >> SPI2_Init

  I2S_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_ITConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_DMACmd (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text))
  [Called By]

  - >> DMA1_Spi2_Init
  - >> DMA1_Spi1_Init

  SPI_I2S_SendData (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text))
  [Called By]

  - >> SPI1_ReadWriteByte
  - >> SPI2_ReadWriteByte

  SPI_I2S_ReceiveData (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text))
  [Called By]

  - >> SPI1_ReadWriteByte
  - >> SPI2_ReadWriteByte

  SPI_NSSInternalSoftwareConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_SSOutputCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_DataSizeConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_TransmitCRC (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_CalculateCRC (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_GetCRC (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_GetCRCPolynomial (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_BiDirectionalLineConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_GetFlagStatus (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text))
  [Called By]

  - >> SPI1_ReadWriteByte
  - >> SPI2_ReadWriteByte

  SPI_I2S_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_GetITStatus (Thumb, 44 bytes, Stack size 12 bytes, stm32f10x_spi.o(.text), UNUSED)

  SPI_I2S_ClearITPendingBit (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_spi.o(.text), UNUSED)

  DMA_DeInit (Thumb, 218 bytes, Stack size 0 bytes, stm32f10x_dma.o(.text))
  [Called By]

  - >> DMA1_Spi2_Init
  - >> DMA1_Spi1_Init
  - >> USART1_RX_DMA_Init

  DMA_Init (Thumb, 58 bytes, Stack size 12 bytes, stm32f10x_dma.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = DMA_Init
  [Called By]
  - >> DMA1_Spi2_Init
  - >> DMA1_Spi1_Init
  - >> USART1_RX_DMA_Init

  DMA_StructInit (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_dma.o(.text), UNUSED)

  DMA_Cmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_dma.o(.text))
  [Called By]

  - >> DMA1_Spi2_TX
  - >> DMA1_Spi2_RX
  - >> DMA1_Spi1_TX
  - >> DMA1_Spi1_RX
  - >> USART1_RX_DMA_Init

  DMA_ITConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_dma.o(.text))
  [Called By]

  - >> USART1_RX_DMA_Init

  DMA_SetCurrDataCounter (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_dma.o(.text), UNUSED)

  DMA_GetCurrDataCounter (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_dma.o(.text), UNUSED)

  DMA_GetFlagStatus (Thumb, 28 bytes, Stack size 0 bytes, stm32f10x_dma.o(.text))
  [Called By]

  - >> DMA1_Spi2_TX
  - >> DMA1_Spi2_RX
  - >> DMA1_Spi1_TX
  - >> DMA1_Spi1_RX

  DMA_ClearFlag (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_dma.o(.text))
  [Called By]

  - >> DMA1_Spi2_TX
  - >> DMA1_Spi2_RX
  - >> DMA1_Spi1_TX
  - >> DMA1_Spi1_RX
  - >> USART1_RX_DMA_Init

  DMA_GetITStatus (Thumb, 28 bytes, Stack size 0 bytes, stm32f10x_dma.o(.text), UNUSED)

  DMA_ClearITPendingBit (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_dma.o(.text))
  [Called By]

  - >> DMA1_Channel5_IRQHandler

  TIM_DeInit (Thumb, 304 bytes, Stack size 8 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB1PeriphResetCmd
  - >> RCC_APB2PeriphResetCmd

  TIM_TimeBaseInit (Thumb, 114 bytes, Stack size 12 bytes, stm32f10x_tim.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_TimeBaseInit
  [Called By]
  - >> TIM3_Int_Init

  TIM_OC1Init (Thumb, 106 bytes, Stack size 12 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC2Init (Thumb, 120 bytes, Stack size 16 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC3Init (Thumb, 116 bytes, Stack size 16 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC4Init (Thumb, 90 bytes, Stack size 16 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SetIC4Prescaler (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ICInit

  TIM_SetIC3Prescaler (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ICInit

  TIM_SetIC2Prescaler (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  TIM_SetIC1Prescaler (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  TIM_ICInit (Thumb, 270 bytes, Stack size 40 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SetIC1Prescaler
  - >> TIM_SetIC2Prescaler
  - >> TIM_SetIC3Prescaler
  - >> TIM_SetIC4Prescaler
  - >> TI1_Config
  - >> TI2_Config

  TIM_PWMIConfig (Thumb, 104 bytes, Stack size 24 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SetIC1Prescaler
  - >> TIM_SetIC2Prescaler
  - >> TI1_Config
  - >> TI2_Config

  TIM_BDTRConfig (Thumb, 34 bytes, Stack size 8 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_TimeBaseStructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OCStructInit (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ICStructInit (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_BDTRStructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text))
  [Called By]

  - >> TIM3_Int_Init

  TIM_CtrlPWMOutputs (Thumb, 22 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ITConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text))
  [Called By]

  - >> TIM3_Int_Init

  TIM_GenerateEvent (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_DMAConfig (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_DMACmd (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_InternalClockConfig (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectInputTrigger (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_TIxExternalClockConfig
  - >> TIM_ITRxExternalClockConfig

  TIM_ITRxExternalClockConfig (Thumb, 18 bytes, Stack size 4 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SelectInputTrigger

  TIM_TIxExternalClockConfig (Thumb, 46 bytes, Stack size 16 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SelectInputTrigger
  - >> TI1_Config
  - >> TI2_Config

  TIM_ETRConfig (Thumb, 24 bytes, Stack size 12 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ETRClockMode2Config
  - >> TIM_ETRClockMode1Config

  TIM_ETRClockMode1Config (Thumb, 18 bytes, Stack size 8 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_ETRConfig

  TIM_ETRClockMode2Config (Thumb, 18 bytes, Stack size 8 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_ETRConfig

  TIM_PrescalerConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_CounterModeConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_EncoderInterfaceConfig (Thumb, 50 bytes, Stack size 16 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ForcedOC1Config (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ForcedOC2Config (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ForcedOC3Config (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ForcedOC4Config (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ARRPreloadConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectCOM (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectCCDMA (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_CCPreloadControl (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC1PreloadConfig (Thumb, 32 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC2PreloadConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC3PreloadConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC4PreloadConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC1FastConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC2FastConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC3FastConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC4FastConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ClearOC1Ref (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ClearOC2Ref (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ClearOC3Ref (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ClearOC4Ref (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC1PolarityConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC1NPolarityConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC2PolarityConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC2NPolarityConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC3PolarityConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC3NPolarityConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_OC4PolarityConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_CCxCmd (Thumb, 22 bytes, Stack size 8 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_CCxNCmd (Thumb, 22 bytes, Stack size 8 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectOCxM (Thumb, 70 bytes, Stack size 12 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_UpdateDisableConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_UpdateRequestConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectHallSensor (Thumb, 20 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectOnePulseMode (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectOutputTrigger (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectSlaveMode (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SelectMasterSlaveMode (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SetCounter (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SetAutoreload (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SetCompare1 (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SetCompare2 (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SetCompare3 (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SetCompare4 (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_SetClockDivision (Thumb, 16 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_GetCapture1 (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_GetCapture2 (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_GetCapture3 (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_GetCapture4 (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_GetCounter (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_GetPrescaler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_GetFlagStatus (Thumb, 14 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text), UNUSED)

  TIM_GetITStatus (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text))
  [Called By]

  - >> TIM3_IRQHandler

  TIM_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(.text))
  [Called By]

  - >> TIM3_IRQHandler

  image_getcolor (Thumb, 20 bytes, Stack size 0 bytes, image2lcd.o(.text))
  [Called By]

  - >> image_show

  image_show (Thumb, 68 bytes, Stack size 24 bytes, image2lcd.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = image_show ⇒ LCD_Set_Window ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> LCD_Set_Window
  - >> LCD_WriteRAM_Prepare
  - >> LCD_WriteRAM
  - >> image_getcolor
  [Called By]
  - >> image_display

  image_display (Thumb, 22 bytes, Stack size 16 bytes, image2lcd.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = image_display ⇒ image_show ⇒ LCD_Set_Window ⇒ LCD_WR_DATA ⇒ SPI2_ReadWriteByte
  [Calls]
  - >> image_show
  [Called By]
  - >> LCD_Init

  USART1_RX_DMA_Init (Thumb, 144 bytes, Stack size 64 bytes, updater.o(.text))
  [Stack]

  - Max Depth = 76
  - Call Chain = USART1_RX_DMA_Init ⇒ NVIC_Init
  [Calls]
  - >> USART_DMACmd
  - >> NVIC_Init
  - >> RCC_AHBPeriphClockCmd
  - >> DMA_Init
  - >> DMA_DeInit
  - >> DMA_Cmd
  - >> DMA_ClearFlag
  - >> DMA_ITConfig
  [Called By]
  - >> Update
  - >> DMA1_Channel5_IRQHandler

  DMA1_Channel5_IRQHandler (Thumb, 84 bytes, Stack size 8 bytes, updater.o(.text))
  [Stack]

  - Max Depth = 84
  - Call Chain = DMA1_Channel5_IRQHandler ⇒ USART1_RX_DMA_Init ⇒ NVIC_Init
  [Calls]
  - >> USART1_RX_DMA_Init
  - >> DMA_ClearITPendingBit
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  TIM3_Int_Init (Thumb, 90 bytes, Stack size 32 bytes, updater.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = TIM3_Int_Init ⇒ NVIC_Init
  [Calls]
  - >> NVIC_Init
  - >> RCC_APB1PeriphClockCmd
  - >> TIM_ITConfig
  - >> TIM_Cmd
  - >> TIM_TimeBaseInit
  [Called By]
  - >> main

  TIM3_IRQHandler (Thumb, 38 bytes, Stack size 8 bytes, updater.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM3_IRQHandler
  [Calls]
  - >> TIM_ClearITPendingBit
  - >> TIM_GetITStatus
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  sun (Thumb, 22 bytes, Stack size 16 bytes, updater.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = sun
  [Called By]
  - >> NVIC_PriorityGroupConfigSet
  - >> Update

  Update (Thumb, 446 bytes, Stack size 24 bytes, updater.o(.text), UNUSED)
  [Calls]

  - >> W25QXX_Erase_Chip
  - >> W25QXX_Write_NoCheck
  - >> W25QXX_Write
  - >> W25QXX_Read
  - >> SendPWMval
  - >> LCD_ShowString
  - >> __2printf
  - >> sun
  - >> USART1_RX_DMA_Init

  Sys_Soft_Reset (Thumb, 20 bytes, Stack size 0 bytes, updater.o(.text))
  [Called By]

  - >> NVIC_PriorityGroupConfigSet

  NVIC_PriorityGroupConfigSet (Thumb, 682 bytes, Stack size 32 bytes, updater.o(.text))
  [Stack]

  - Max Depth = 164
  - Call Chain = NVIC_PriorityGroupConfigSet ⇒ W25QXX_Init ⇒ SPI1_Init ⇒ DMA1_Spi1_Init ⇒ DMA_Init
  [Calls]
  - >> W25QXX_Write
  - >> W25QXX_Read
  - >> uart_init
  - >> delay_ms
  - >> W25QXX_Init
  - >> TIM2_PWM_Init
  - >> SendPWMval
  - >> LCD_Init
  - >> LCD_Clear
  - >> Sys_Soft_Reset
  - >> sun
  [Called By]
  - >> NVIC_Configuration

  strlen (Thumb, 14 bytes, Stack size 0 bytes, strlen.o(.text), UNUSED)
  [Called By]

  - >> Show_Str_Mid

  strcmp (Thumb, 28 bytes, Stack size 8 bytes, strcmp.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = strcmp
  [Called By]
  - >> GT911_Init

  __aeabi_fadd (Thumb, 164 bytes, Stack size 16 bytes, fadd.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = __aeabi_fadd ⇒ _float_epilogue
  [Calls]
  - >> _float_round
  - >> _float_epilogue
  [Called By]
  - >> __aeabi_fsub
  - >> TP_Scan
  - >> __aeabi_frsub

  __aeabi_fsub (Thumb, 6 bytes, Stack size 0 bytes, fadd.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = __aeabi_fsub ⇒ __aeabi_fadd ⇒ _float_epilogue
  [Calls]
  - >> __aeabi_fadd
  [Called By]
  - >> TP_Adjust

  __aeabi_frsub (Thumb, 6 bytes, Stack size 0 bytes, fadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_fadd

  __aeabi_fmul (Thumb, 100 bytes, Stack size 8 bytes, fmul.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_fmul
  [Called By]
  - >> TP_Adjust
  - >> TP_Save_Adjdata
  - >> TP_Scan

  __aeabi_fdiv (Thumb, 124 bytes, Stack size 8 bytes, fdiv.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_fdiv
  [Calls]
  - >> _float_round
  [Called By]
  - >> TP_Adjust
  - >> TP_Get_Adjdata

  __ARM_scalbnf (Thumb, 24 bytes, Stack size 0 bytes, fscalb.o(.text))
  [Called By]

  - >> TP_Adjust

  scalbnf (Thumb, 0 bytes, Stack size 0 bytes, fscalb.o(.text), UNUSED)

  __aeabi_dmul (Thumb, 228 bytes, Stack size 48 bytes, dmul.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> TP_Adjust
  - >> _fp_digits

  __aeabi_i2f (Thumb, 18 bytes, Stack size 0 bytes, fflti.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = __aeabi_i2f ⇒ _float_epilogue
  [Calls]
  - >> _float_epilogue
  [Called By]
  - >> TP_Adjust
  - >> TP_Get_Adjdata
  - >> TP_Scan

  __aeabi_ui2f (Thumb, 10 bytes, Stack size 0 bytes, ffltui.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = __aeabi_ui2f ⇒ _float_epilogue
  [Calls]
  - >> _float_epilogue
  [Called By]
  - >> TP_Adjust
  - >> TP_Scan

  __aeabi_ui2d (Thumb, 26 bytes, Stack size 16 bytes, dfltui.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = __aeabi_ui2d ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> TP_Adjust

  __aeabi_f2iz (Thumb, 50 bytes, Stack size 0 bytes, ffixi.o(.text))
  [Called By]

  - >> TP_Adjust
  - >> TP_Save_Adjdata

  __aeabi_f2uiz (Thumb, 40 bytes, Stack size 0 bytes, ffixui.o(.text))
  [Called By]

  - >> TP_Scan

  __aeabi_d2uiz (Thumb, 50 bytes, Stack size 8 bytes, dfixui.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_d2uiz
  [Calls]
  - >> __aeabi_llsr
  [Called By]
  - >> TP_Adjust

  __aeabi_f2d (Thumb, 38 bytes, Stack size 0 bytes, f2d.o(.text))
  [Called By]

  - >> TP_Adjust

  __aeabi_cdcmpeq (Thumb, 0 bytes, Stack size 0 bytes, cdcmple.o(.text), UNUSED)

  __aeabi_cdcmple (Thumb, 48 bytes, Stack size 0 bytes, cdcmple.o(.text))
  [Called By]

  - >> TP_Adjust

  __aeabi_cdrcmple (Thumb, 48 bytes, Stack size 0 bytes, cdrcmple.o(.text))
  [Called By]

  - >> TP_Adjust
  - >> _fp_digits

  __aeabi_uidiv (Thumb, 0 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)

  __aeabi_uidivmod (Thumb, 44 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)
  [Called By]

  - >> _printf_core

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsl
  - >> __aeabi_llsr
  [Called By]
  - >> _printf_core
  - >> _fp_digits

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text))
  [Called By]

  - >> __aeabi_d2uiz
  - >> __aeabi_d2ulz
  - >> _dsqrt
  - >> __aeabi_uldivmod
  - >> _double_epilogue

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  __I$use$fp (Thumb, 0 bytes, Stack size 0 bytes, iusefp.o(.text), UNUSED)

  _float_round (Thumb, 18 bytes, Stack size 0 bytes, fepilogue.o(.text))
  [Called By]

  - >> __aeabi_fdiv
  - >> __aeabi_fadd

  _float_epilogue (Thumb, 92 bytes, Stack size 4 bytes, fepilogue.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = _float_epilogue
  [Called By]
  - >> __aeabi_ui2f
  - >> __aeabi_i2f
  - >> __aeabi_fadd

  _double_round (Thumb, 30 bytes, Stack size 8 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = _double_round
  [Called By]
  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> _dsqrt
  - >> _double_epilogue

  _double_epilogue (Thumb, 156 bytes, Stack size 32 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_llsl
  - >> _double_round
  - >> __aeabi_llsr
  [Called By]
  - >> __aeabi_ui2d
  - >> __aeabi_dmul
  - >> __aeabi_dadd

  __aeabi_dadd (Thumb, 322 bytes, Stack size 48 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_lasr
  - >> __aeabi_llsl
  - >> _double_round
  - >> _double_epilogue
  [Called By]
  - >> _fp_digits
  - >> __aeabi_drsub
  - >> __aeabi_dsub

  __aeabi_dsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_dadd

  __aeabi_drsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_dadd

  __aeabi_ddiv (Thumb, 222 bytes, Stack size 32 bytes, ddiv.o(.text), UNUSED)
  [Calls]

  - >> _double_round
  [Called By]
  - >> _fp_digits

  _dsqrt (Thumb, 162 bytes, Stack size 32 bytes, dsqrt.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _dsqrt ⇒ _double_round
  [Calls]
  - >> _double_round
  - >> __aeabi_llsr
  [Called By]
  - >> sqrt

  __aeabi_d2ulz (Thumb, 48 bytes, Stack size 0 bytes, dfixul.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsl
  - >> __aeabi_llsr
  [Called By]
  - >> _fp_digits

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text))
  [Called By]

  - >> __aeabi_dadd
  - >> __aeabi_d2ulz
  - >> __aeabi_uldivmod
  - >> _double_epilogue

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_lasr (Thumb, 36 bytes, Stack size 0 bytes, llsshr.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_dadd

  _ll_sshift_r (Thumb, 0 bytes, Stack size 0 bytes, llsshr.o(.text), UNUSED)

  __0printf (Thumb, 22 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)
  [Calls]

  - >> _printf_core

  __1printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)

  __2printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2printf
  [Called By]
  - >> GT911_Scan
  - >> GT911_Init
  - >> CST3XX_Scan
  - >> TP_Adjust
  - >> TP_Get_Adjdata
  - >> TP_Scan
  - >> ctp_test
  - >> W25QXX_Init
  - >> main
  - >> Update

  __c89printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)

  printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  __set_errno (Thumb, 6 bytes, Stack size 0 bytes, errno.o(i.__set_errno))
  [Called By]

  - >> sqrt

  free (Thumb, 76 bytes, Stack size 8 bytes, malloc.o(i.free))
  [Stack]

  - Max Depth = 8
  - Call Chain = free
  [Called By]
  - >> text_show_font
  - >> main

  malloc (Thumb, 92 bytes, Stack size 20 bytes, malloc.o(i.malloc))
  [Stack]

  - Max Depth = 20
  - Call Chain = malloc
  [Called By]
  - >> text_show_font

  sqrt (Thumb, 76 bytes, Stack size 24 bytes, sqrt.o(i.sqrt))
  [Stack]

  - Max Depth = 64
  - Call Chain = sqrt ⇒ _dsqrt ⇒ _double_round
  [Calls]
  - >> _dsqrt
  - >> __set_errno
  [Called By]
  - >> TP_Adjust

  ### Local Symbols

  SetSysClockTo72 (Thumb, 160 bytes, Stack size 12 bytes, system_stm32f10x.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClockTo72
  [Called By]
  - >> SystemInit

  text_get_hz_mat (Thumb, 130 bytes, Stack size 8 bytes, text.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = text_get_hz_mat ⇒ W25QXX_Read ⇒ DMA1_Spi1_RX
  [Calls]
  - >> W25QXX_Read
  [Called By]
  - >> text_show_font

  TI2_Config (Thumb, 166 bytes, Stack size 20 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_TIxExternalClockConfig
  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  TI1_Config (Thumb, 88 bytes, Stack size 16 bytes, stm32f10x_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_TIxExternalClockConfig
  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  _fp_digits (Thumb, 334 bytes, Stack size 56 bytes, printfa.o(i._fp_digits), UNUSED)
  [Calls]

  - >> __aeabi_dmul
  - >> __aeabi_cdrcmple
  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> __aeabi_d2ulz
  - >> __aeabi_uldivmod
  [Called By]
  - >> _printf_core

  _printf_core (Thumb, 1744 bytes, Stack size 136 bytes, printfa.o(i._printf_core), UNUSED)
  [Calls]

  - >> _printf_pre_padding
  - >> _printf_post_padding
  - >> _fp_digits
  - >> __aeabi_uldivmod
  - >> __aeabi_uidivmod
  [Called By]
  - >> __0printf

  _printf_post_padding (Thumb, 36 bytes, Stack size 24 bytes, printfa.o(i._printf_post_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _printf_pre_padding (Thumb, 46 bytes, Stack size 24 bytes, printfa.o(i._printf_pre_padding), UNUSED)
  [Called By]

  - >> _printf_core

  ### Undefined Global Symbols